Inductive sensor; Sensing range 40 mm non-flush mountable; Operating voltage 10...36 DC V; 3-wire; PNP; M12 Connector
Product designation	Inductive sensor
Operating voltage DC	10...36 V
Voltage type	DC
Electrical design	PNP
Output function	normally open
Mounting	non-flush mountable
Connection	M12 Connector
Materials	housing: PA; sensing face: PA black; bevelled housing part: PA; clamp: orange; screw: stainless steel (304CU/1.4567)
Display	switching status: 1 x LED yellow; operation: 1 x LED green
Ambient temperature	-25...70 °C
Brand	ifm electronic gmbh or equivalent
Type	IM5117